#MicroXplorer Configuration settings - do not modify
File.Version=6
GPIO.groupedBy=Group By Peripherals
KeepUserPlacement=false
Mcu.CPN=STM32F769NIH6
Mcu.Family=STM32F7
Mcu.IP0=CORTEX_M7
Mcu.IP1=NVIC
Mcu.IP2=RCC
Mcu.IP3=SYS
Mcu.IP4=TIM1
Mcu.IP5=USART1
Mcu.IPNb=6
Mcu.Name=STM32F769NIHx
Mcu.Package=TFBGA216
Mcu.Pin0=PB9
Mcu.Pin1=PJ13
Mcu.Pin2=PA10
Mcu.Pin3=PA9
Mcu.Pin4=PH0/OSC_IN
Mcu.Pin5=PH1/OSC_OUT
Mcu.Pin6=PD14
Mcu.Pin7=VP_SYS_VS_Systick
Mcu.Pin8=VP_TIM1_VS_ClockSourceINT
Mcu.PinsNb=9
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32F769NIHx
MxCube.Version=6.5.0
MxDb.Version=DB.6.0.50
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true
NVIC.SysTick_IRQn=true\:15\:0\:false\:false\:true\:false\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true
PA10.Locked=true
PA10.Mode=Asynchronous
PA10.Signal=USART1_RX
PA9.Locked=true
PA9.Mode=Asynchronous
PA9.Signal=USART1_TX
PB9.GPIOParameters=GPIO_Speed,PinState
PB9.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PB9.Locked=true
PB9.PinState=GPIO_PIN_SET
PB9.Signal=GPIO_Output
PD14.Locked=true
PD14.Signal=GPIO_Output
PH0/OSC_IN.Mode=HSE-External-Oscillator
PH0/OSC_IN.Signal=RCC_OSC_IN
PH1/OSC_OUT.Mode=HSE-External-Oscillator
PH1/OSC_OUT.Signal=RCC_OSC_OUT
PJ13.Locked=true
PJ13.Signal=GPIO_Output
PinOutPanel.CurrentBGAView=Top
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32F769NIHx
ProjectManager.FirmwarePackage=STM32Cube FW_F7 V1.16.2
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=dhry_03_09.ioc
ProjectManager.ProjectName=dhry_03_09
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-false-HAL-false,2-MX_GPIO_Init-GPIO-false-HAL-true,3-MX_USART1_UART_Init-USART1-false-HAL-true,4-MX_TIM1_Init-TIM1-false-HAL-true,0-MX_CORTEX_M7_Init-CORTEX_M7-false-HAL-true
RCC.AHBFreq_Value=215384615.38461536
RCC.APB1CLKDivider=RCC_HCLK_DIV4
RCC.APB1Freq_Value=53846153.84615384
RCC.APB1TimFreq_Value=107692307.69230768
RCC.APB2CLKDivider=RCC_HCLK_DIV2
RCC.APB2Freq_Value=107692307.69230768
RCC.APB2TimFreq_Value=215384615.38461536
RCC.CECFreq_Value=32786.88524590164
RCC.CortexFreq_Value=215384615.38461536
RCC.DFSDMAudioFreq_Value=184615384.6153846
RCC.DFSDMFreq_Value=107692307.69230768
RCC.DSIFreq_Value=62500000
RCC.DSITXEscFreq_Value=15625000
RCC.EthernetFreq_Value=215384615.38461536
RCC.FCLKCortexFreq_Value=215384615.38461536
RCC.FamilyName=M
RCC.HCLKFreq_Value=215384615.38461536
RCC.HSE_VALUE=25000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=53846153.84615384
RCC.I2C2Freq_Value=53846153.84615384
RCC.I2C3Freq_Value=53846153.84615384
RCC.I2C4Freq_Value=53846153.84615384
RCC.I2SFreq_Value=184615384.6153846
RCC.IPParameters=AHBFreq_Value,APB1CLKDivider,APB1Freq_Value,APB1TimFreq_Value,APB2CLKDivider,APB2Freq_Value,APB2TimFreq_Value,CECFreq_Value,CortexFreq_Value,DFSDMAudioFreq_Value,DFSDMFreq_Value,DSIFreq_Value,DSITXEscFreq_Value,EthernetFreq_Value,FCLKCortexFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2C4Freq_Value,I2SFreq_Value,LCDTFTFreq_Value,LPTIM1Freq_Value,LSE_VALUE,LSI_VALUE,MCO2PinFreq_Value,PLLCLKFreq_Value,PLLDSIVCOFreq_Value,PLLI2SPCLKFreq_Value,PLLI2SQCLKFreq_Value,PLLI2SRCLKFreq_Value,PLLI2SRoutputFreq_Value,PLLM,PLLN,PLLQCLKFreq_Value,PLLQoutputFreq_Value,PLLRFreq_Value,PLLSAIPCLKFreq_Value,PLLSAIQCLKFreq_Value,PLLSAIRCLKFreq_Value,PLLSAIoutputFreq_Value,PLLSourceVirtual,RNGFreq_Value,SAI1Freq_Value,SAI2Freq_Value,SDMMC2Freq_Value,SDMMCFreq_Value,SPDIFRXFreq_Value,SYSCLKFreq_VALUE,SYSCLKSource,UART4Freq_Value,UART5Freq_Value,UART7Freq_Value,UART8Freq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USART6Freq_Value,USBFreq_Value,VCOI2SOutputFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VCOSAIOutputFreq_Value
RCC.LCDTFTFreq_Value=92307692.3076923
RCC.LPTIM1Freq_Value=53846153.84615384
RCC.LSE_VALUE=32768
RCC.LSI_VALUE=32000
RCC.MCO2PinFreq_Value=215384615.38461536
RCC.PLLCLKFreq_Value=215384615.38461536
RCC.PLLDSIVCOFreq_Value=1000000000
RCC.PLLI2SPCLKFreq_Value=184615384.6153846
RCC.PLLI2SQCLKFreq_Value=184615384.6153846
RCC.PLLI2SRCLKFreq_Value=184615384.6153846
RCC.PLLI2SRoutputFreq_Value=184615384.6153846
RCC.PLLM=13
RCC.PLLN=224
RCC.PLLQCLKFreq_Value=215384615.38461536
RCC.PLLQoutputFreq_Value=215384615.38461536
RCC.PLLRFreq_Value=215384615.38461536
RCC.PLLSAIPCLKFreq_Value=184615384.6153846
RCC.PLLSAIQCLKFreq_Value=184615384.6153846
RCC.PLLSAIRCLKFreq_Value=184615384.6153846
RCC.PLLSAIoutputFreq_Value=184615384.6153846
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.RNGFreq_Value=215384615.38461536
RCC.SAI1Freq_Value=184615384.6153846
RCC.SAI2Freq_Value=184615384.6153846
RCC.SDMMC2Freq_Value=215384615.38461536
RCC.SDMMCFreq_Value=215384615.38461536
RCC.SPDIFRXFreq_Value=184615384.6153846
RCC.SYSCLKFreq_VALUE=215384615.38461536
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.UART4Freq_Value=53846153.84615384
RCC.UART5Freq_Value=53846153.84615384
RCC.UART7Freq_Value=53846153.84615384
RCC.UART8Freq_Value=53846153.84615384
RCC.USART1Freq_Value=107692307.69230768
RCC.USART2Freq_Value=53846153.84615384
RCC.USART3Freq_Value=53846153.84615384
RCC.USART6Freq_Value=107692307.69230768
RCC.USBFreq_Value=215384615.38461536
RCC.VCOI2SOutputFreq_Value=369230769.2307692
RCC.VCOInputFreq_Value=1923076.923076923
RCC.VCOOutputFreq_Value=430769230.7692307
RCC.VCOSAIOutputFreq_Value=369230769.2307692
TIM1.IPParameters=Prescaler
TIM1.Prescaler=107
USART1.IPParameters=VirtualMode-Asynchronous
USART1.VirtualMode-Asynchronous=VM_ASYNC
VP_SYS_VS_Systick.Mode=SysTick
VP_SYS_VS_Systick.Signal=SYS_VS_Systick
VP_TIM1_VS_ClockSourceINT.Mode=Internal
VP_TIM1_VS_ClockSourceINT.Signal=TIM1_VS_ClockSourceINT
board=custom
isbadioc=false
