../Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_hal_uart_ex.c:745:13:UARTEx_Wakeup_AddressConfig.isra	4	static
../Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_hal_uart_ex.c:150:19:HAL_RS485Ex_Init	24	static
../Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_hal_uart_ex.c:300:19:HAL_UARTEx_EnableClockStopMode	0	static,ignoring_inline_asm
../Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_hal_uart_ex.c:319:19:HAL_UARTEx_DisableClockStopMode	0	static,ignoring_inline_asm
../Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_hal_uart_ex.c:347:19:HAL_MultiProcessorEx_AddressLength_Set	4	static
../Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_hal_uart_ex.c:386:19:HAL_UARTEx_StopModeWakeUpSourceConfig	32	static
../Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_hal_uart_ex.c:443:19:HAL_UARTEx_EnableStopMode	0	static,ignoring_inline_asm
../Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_hal_uart_ex.c:462:19:HAL_UARTEx_DisableStopMode	0	static,ignoring_inline_asm
../Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_hal_uart_ex.c:494:19:HAL_UARTEx_ReceiveToIdle	40	static
../Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_hal_uart_ex.c:619:19:HAL_UARTEx_ReceiveToIdle_IT	16	static,ignoring_inline_asm
../Drivers/STM32F7xx_HAL_Driver/Src/stm32f7xx_hal_uart_ex.c:681:19:HAL_UARTEx_ReceiveToIdle_DMA	16	static,ignoring_inline_asm
