{software_version:01.04}
{boot_mode:3}
{smooth_shutdown_time:0060}
{scheduled_boot_utc_time:08:32:00}
{scheduled_boot_date:05/01/2024}
{gs_contact_waittime_in_min:0020}

________
Readme :
--------
1. Firmware version to be updated

2. Boot mode is the type of firmware update command as given below
   BOOT_NOW       = 1 >> This command will perform firmware update process immediately
   BOOT_POSTPONED = 2 >> Postponed the firmware update process
   BOOT_SCHEDULED = 3 >> Trigger firmware update at scheduled time as given in (scheduled_boot_utc_time) and (scheduled_boot_date)

3. Smooth shutdown waiting time in seconds to shutdown the system before initiate software reset, input should always be in 4 digit field.
   Ex 60 seconds to be given as 0060

4. Schduled boot time in UTC-0 format 

5. Schduled boot date

6. GS contact wait timeout time in minutes, input should be in 4 digit number. example- 23 minutes should be denoted as 0023
